District of Columbia Municipal Regulations


A102
APPLICABILITY AND CONFORMANCE

Strike Section A102.2 in Appendix A of the International Green Construction Code in its entirety and insert new Section A102.2 in Appendix A of the Green Construction Code in its place to read as follows:

A102.2 Required number and selection of project electives. New construction projects shall attain a total of 18 project electives, Level 3 alterations and core-and-shell projects shall attain 13 project electives, first time tenant fit-outs 10,000 square feet and larger shall attain ten project electives, and Level 2 alterations 50,000 square feet and larger, where 10,000 square feet of the space is being reconfigured, shall attain ten project electives. For first-time tenant fit-outs and Level 2 alterations, up to three of the project electives can come from base building features.

Selected project electives shall be applied as mandatory requirements, and shall be communicated to the code official in the manner and form specified by the code official. Electives shall be disallowed if an elective is deemed by the code official not to meet the substantial intent of the elective.

SOURCE: Final Rulemaking published at 67 DCR 6509 (May 29, 2020 – Part 2).
The District of Columbia Green Construction Code (2017), referred to as the “Green Construction Code,” consists of the 2012 edition of the International Green Construction Code (International Green Construction Code), published by the International Code Council (ICC), as amended by the District of Columbia Green Construction Code Supplement  of 2017 (12-K DCMR). The International Green Construction Code is copyrighted by the ICC and therefore is not republished here. However, a copy of the text may be obtained at:
https://codes.iccsafe.org/public/document/toc/548/.
	
	Green Construction Code Supplement of 2017 
12-K DCMR § A102

	

	
	
	



