District of Columbia Municipal Regulations


801
GENERAL

Strike Section 801.2 of the International Green Construction Code in its entirety and insert new Section 801.2 in the Green Construction Code in its place to read as follows:
801.2 Demolition and construction phase indoor air quality management plan required.  An indoor air quality management plan shall be developed and submitted with permit application materials. Such plan shall address the methods and procedures to be used during design and construction to obtain compliance with Sections 802 through 805. 

SOURCE: Final Rulemaking published at 67 DCR 6509 (May 29, 2020 – Part 2).
The District of Columbia Green Construction Code (2017), referred to as the “Green Construction Code,” consists of the 2012 edition of the International Green Construction Code (International Green Construction Code), published by the International Code Council (ICC), as amended by the District of Columbia Green Construction Code Supplement  of 2017 (12-K DCMR). The International Green Construction Code is copyrighted by the ICC and therefore is not republished here. However, a copy of the text may be obtained at:
https://codes.iccsafe.org/public/document/toc/548/.
	
	Green Construction Code Supplement of 2017 
12-K DCMR § 801

	

	
	
	



