District of Columbia Municipal Regulations


402  
DENSITY – FLOOR AREA RATIO (FAR)

402.1
The maximum permitted FAR in the MU-3 through MU-10 zones shall be as set forth in the following table:

TABLE G § 402.1: MAXIMUM PERMITTED FLOOR AREA RATIO

	Zone
	Maximum FAR

	
	Total Permitted
	Maximum 

Non-Residential Use

	MU-3A
	1.0
	1.0

	
	1.2 (IZ)
	

	MU-3B
	2.0
	1.5

	
	2.4 (IZ)
	

	MU-4
	2.5
	1.5

	
	3.0 (IZ)
	

	MU-5-A

MU-5-B
	3.5
	1.5

	
	4.2 (IZ)
	

	MU-6
	6.0
	2.0

	
	7.2 (IZ)
	

	MU-7
	4.0
	2.5

	
	4.8 (IZ)
	

	MU-8
	5.0
	4.0

	
	6.0 (IZ)
	

	MU-9
	6.5
	6.5

	
	7.8 (IZ)
	

	MU-10
	6.0
	3.0

	
	7.2 (IZ)
	


402.1 In the MU-4 and MU-5 zones, an existing building on a lot with an area ten thousand square feet (10,000 sq. ft.) or less, may have a maximum density of 2.0 FAR for non-residential uses, provided the uses are located in the ground story and the story directly above the ground story. For new construction, any additional use is limited to 0.5 FAR.

402.3
In the MU-10 zone, combined lot development is permitted for the purposes of allocating gross floor area devoted to residential and non-residential uses in accordance with the provisions of Subtitle C Chapter 12.  Both lots shall be located within the same square, and shall be zoned MU-10.

402.4 
In the MU-30 zone, the maximum permitted FAR shall be as set forth in the following table:
TABLE G § 402.4: MAXIMUM PERMITTED FAR
	MU-30 Zone Height
	Maximum FAR

	
	Total Permitted
	Maximum 

Non-Residential Use

	Buildings erected to a height of one hundred ten feet (110 ft.) or less
	8.5
	8.5 

	
	10.2 (IZ)
	

	Buildings erected to a height in excess of one hundred ten feet (110 ft.) as permitted in Subtitle G § 403.2
	10.0
	10.0

	
	12.0 (IZ)
	


SOURCE: Final Rulemaking published at 63 DCR 2447, 2944 (March 4, 2016 – Part 2); as amended by Final Rulemaking published at 64 DCR 22 (January 6, 2017); as amended by Final Rulemaking published at 64 DCR 7264 (July 28, 2017); as amended by Final Rulemaking published at 65 DCR 11490 (October 12, 2018).
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