District of Columbia Municipal Regulations


1602  
HEIGHT

1602.1 A public recreation and community center may be erected to a height as follows: 

(a) In an R, RF, or RA zone a public recreation and community center may be erected to a height not to exceed forty-five feet (45 ft.); 

(b) In the RF-3 and MU-11 zone a public recreation and community center may be erected to a height not to exceed forty feet (40 ft.); and 

(c) In all other zones, a public recreation and community center may be erected to the maximum height permitted within the zone.

1602.2 A public library may be built to the maximum height permitted within the zone located. 

1602.3 A college or university building or structure covered by an approved campus plan pursuant to Subtitle X, Chapter 1 may be erected to a height not exceeding sixty feet (60 ft.) in an RA-2, RA-7, RA-8, and RA-9 zone.

SOURCE: Final Rulemaking published at 63 DCR 2447, 2712 (March 4, 2016 – Part 2); as amended by Final Rulemaking published at 67 DCR 3776 (April 3, 2020). 
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