District of Columbia Municipal Regulations


2702
EMERGENCY AND STANDBY POWER SYSTEMS
Strike Section 2702.1.7 of the International Building Code in its entirety and insert new Section 2702.1.7 in its place in the Building Code to read as follows.
2702.1.7 Group I-2 Occupancies. In Group I-2 occupancies located in flood hazard areas established in Section 1612.3, where new essential electrical systems are installed, and where new essential electrical system generators are installed, the systems and generators shall be located and installed in accordance with ASCE 24. Where connections for hookup of temporary generators are provided, the connections shall be located at or above the elevation required in ASCE 24.
SOURCE: Final Rulemaking published at 68 DCR 7439 (July 30, 2021).
The District of Columbia Building Code (2017), referred to as the “Building Code,” consists of the 2015 edition of the International Building Code (International Building Code), published by the International Code Council (ICC), as amended by the Building Code Supplement of 2017 (12-A DCMR). The International Building Code is copyrighted by the ICC and therefore is not republished here. However, a copy of the text may be obtained at: https://codes.iccsafe.org/public/document/IBC2015.
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