District of Columbia Municipal Regulations


N105 
CARBON MONOXIDE DETECTION 

N105.1 General.  Carbon monoxide alarms shall be installed in all home day care occupancies equipped with a fuel burning appliance or an attached garage.  Carbon monoxide alarms shall be installed in accordance with Section R315 of the Residential Code or Section 908.7 of the Fire Code as applicable.

SOURCE: Final Rulemaking published at 67 DCR 6232 (May 29, 2020 – Part 2).

The District of Columbia Fire Code (2017), referred to as the “Fire Code,” consists of the 2015 edition of the International Fire Code (International Fire Code), published by the International Code Council (ICC), as amended by the Fire Code Supplement of 2017 (12-H DCMR). The International Fire Code is copyrighted by the ICC and therefore is not republished here. However, a copy of the text may be reviewed at:

https://codes.iccsafe.org/public/document/IFC2015.
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