District of Columbia Municipal Regulations


707  
GREEN AREA RATIO (RC)

707.1 A minimum green area ratio (GAR) shall be provided for each lot in an RC zone as set forth in the following table pursuant to the conditions and requirements of Subtitle C, Chapter 6:

TABLE K § 707.1:  MINIMUM GREEN AREA RATIO

	Zone
	Minimum GAR

	RC-1
	0.40

	RC-2
	0.30

	RC-3
	0.30


SOURCE: Final Rulemaking published at 63 DCR 2447, 3176 (March 4, 2016 – Part 2).
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