District of Columbia Municipal Regulations


1700
MINIMUM OCTANE LEVELS

1700.1
Octane levels where automotive fuel is offered for sale or use shall meet the following minimum standards:

(a)
Automotive fuel advertised at an octane rating of 87 shall measure at an octane level of 86.5 or higher;

(b)
Automotive fuel advertised at an octane rating of 89 shall measure at an octane level of 88.5 or higher;

(c)
Automotive fuel advertised at an octane rating of 93 shall measure at an octane level of 92.5 or higher;

(d)
Automotive fuel advertised at an octane rating of 94 shall measure at an octane level of 93.5 or higher.

SOURCE: Final Rulemaking published at 63 DCR 4071 (March 18, 2016).
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