District of Columbia Municipal Regulations


1814
WELL CONSTRUCTION REQUIREMENTS: DRILLING FLUIDS

1814.1
Only potable water shall be used to create a water-based drilling fluid.  

1814.2
The use of a drilling fluid containing additives shall only be permitted if:

(a)
Use of the additive is approved by the Department in the well construction building permit application;

(b)
The additive is used in accordance with manufacture’s recommendations; and

(c)
The additive does not pose a hazard to public health and safety or the environment.

Source: Final Rulemaking published at 63 DCR 13424 (October 28, 2016).
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