755
FEDERAL TRANSIENT EMISSIONS TEST: EQUIPMENT

755.1
Approved engine emission analyzers and related equipment used to perform the tailpipe exhaust emissions portion of the federal transient emissions test shall meet the performance standards established in 40 CFR Parts 51, 85, and 86 or a U.S. Environmental Protection Agency approved equivalent.
755.2
Approved test equipment used to perform the evaporative systems integrity portion of the federal transient emissions test shall meet the performance standards established in 40 CFR Parts 51, 85, and 86 or a U.S. Environmental protection Agency approved equivalent. 

755.3
Approved engine emission analyzers used to perform the idle tailpipe exhaust emissions portion of the federal transient emissions test shall meet the performance standards established in the California Bureau of Automotive Repairs (BAR) 90 specifications, as specified in 40 CFR Part 51, Appendix D.

