District of Columbia Municipal Regulations


770
HEIGHT OF BUILDINGS OR STRUCTURES (C)

770.1
Except as provided in this section and in Chapters 17 and 20 through 25 of this title, the height of a building or structure, not including a penthouse, in a Commercial District shall not exceed that set forth in the following table:

	ZONE DISTRICT
	MAXIMUM
HEIGHT
(Feet)
	MAXIMUM
HEIGHT
(Stories)

	C-1
	40
	3

	C-2-A
	50
	No Limit

	C-2-B,C-3-A
	65
	No Limit

	C-3-B
	70
	6

	C-2-B-1
	75
	No Limit

	C-2-C,C-3-C
	90
	No Limit

	C-4
	110
	No Limit

	C-5(PAD)
	130
	No Limit


770.2
The height of buildings or structures specified in § 770.1 may be exceeded in the instances provided in §§ 770.3 through 770.9.

770.3
Spires, towers, domes, pinnacles or minarets serving as architectural embellishments, penthouses, ventilator shafts, antennas, chimneys, smokestacks, or fire sprinkler tanks may be erected to a height in excess of that which this sections otherwise authorizes. This section shall not be interpreted to bypass otherwise required special exception reviews.

770.4
In the C-4 District, a building or other structure may be erected to a height not exceeding one hundred thirty feet (130 ft.); provided, that the building or other structure shall face or abut a street not less than one hundred ten feet (110 ft.) wide between building lines.

770.5
In the C-5 (PAD) District, a building or other structure may be erected to a height not exceeding one hundred sixty feet (160 ft.); provided:

(a)
The height of the building or structure shall be measured only from the Pennsylvania Avenue curb at the middle of the front of the building or other structure to the highest point of the roof or parapet exclusive of any structure on the roof; and

(b)
That portion of the building or other structure that exceeds one hundred thirty-five feet (135 ft.) in height shall be set back a minimum of fifty feet (50 ft.) from the building line along Pennsylvania Avenue.

770.6
A penthouse may be erected to a height in excess of that which this section otherwise authorizes but shall not exceed the height, as measured from the surface of the roof upon which the penthouse is located, in the following table:

	ZONE DISTRICT
	MAXIMUM PENTHOUSE HEIGHT
	MAXIMUM PENTHOUSE STORIES

	C-1, C-2-A
	12 ft. except 15 ft. for penthouse mechanical space
	1; second story permitted for penthouse mechanical space

	C-2-B, C-3-A
	12 ft. except 18 ft. 6 in. for penthouse mechanical space
	1; second story permitted for penthouse mechanical space

	C-2-B-1, C-3-B
	20 ft.
	1; second story permitted for penthouse mechanical space

	C-2-C; C-3-C; C-4; C-5
	20 ft.
	1 plus mezzanine; second story permitted for penthouse mechanical space


770.7
[REPEALED].
770.8
[REPEALED].
770.9
The height permitted for a building eligible for the additional density permitted pursuant to § 771.4 shall be that permitted by the Act to Regulate the Height of Buildings in the District of Columbia, approved June 1, 1910 (36 Stat. 452, as amended; D.C. Official Code §§ 6-601.01 to 6-601.09).

SOURCE: §§ 5201.1, 5201.2, and 5201.3 of the Zoning Regulations, effective May 12, 1958; as amended by Final Rulemaking published at 27 DCR 2226, 2227 (May 23, 1980); as amended by Final Rulemaking published at 33 DCR 3975, 3978 (July 4, 1986); as amended by Final Rulemaking published at 36 DCR 1509, 1523 (February 24, 1989); as amended by Final Rulemaking published at 47 DCR 9741-43 (December 8, 2000), incorporating by reference the text of Proposed Rulemaking published at 47 DCR 8335, 8409-10 (October 20, 2000); as amended by Final Rulemaking published at 55 DCR 34 (January 4, 2008); as amended by Final Rulemaking published at 57 DCR 3492 (April 23, 2010); as amended by Final Rulemaking published at 62 DCR 5190 (April 24, 2015); as amended by Final Rulemaking published at 63 DCR 390 (January 8, 2016).
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