District of Columbia Municipal Regulations


3542 PLANNED UNIT DEVELOPMENTS (WR)

3542.1 A planned unit development (PUD) in the WR zone shall be subject to the following provisions in addition to the provisions of Chapter 24 of this title:
(a) The minimum area required for a proposed PUD shall be fifteen thousand square feet (15,000 sq. ft.);
(b) In the WR-1, WR-5, WR-6, WR-7, and WR-8 zones, the height, number of stories, and FAR provided in the relevant zone’s development standards table shall serve as the maximum permitted for a PUD; and
(c) In the WR-2, WR-3, and WR-4 zones, the maximum height and FAR limits for PUDs in the WR zone shall be the following:
(1) For the WR-2 zone, the limits on height, number of stories and FAR provided in the development standards table in § 3502 may be increased by no more than ten feet (10 ft.), one (1) story, and twenty percent (20%) FAR;

(2) For the WR-3 zone, the limits on height, number of stories and FAR provided in the development standards table in § 3503 may be increased by no more than ten feet (10 ft.), one (1) story, and twenty percent (20%) FAR; and
(3) For the WR-4 zone, the limits on height, number of stories and FAR provided in the development standards table in § 3504 may be increased by no more than ten feet (10 ft.), one (1) story, and twenty percent (20%) FAR.

SOURCE: Final Rulemaking published at 62 DCR 12168 (September 4, 2015).
	
	Zoning
11 DCMR § 3542

	

	
	
	



