605
CLEANABILITY ─ FLOORS, WALLS, CEILINGS, AND UTILITY LINES  

605.1
Utility service lines and pipes shall not be unnecessarily exposed.  

605.2
Exposed utility service lines and pipes shall be installed so they do not obstruct or prevent cleaning of the floors, walls, or ceilings.  

605.3
Exposed horizontal utility service lines and pipes shall not be installed on the floor.  
SOURCE: Final Rulemaking published at 60 DCR 3582 (March 15, 2013).
