District of Columbia Municipal Regulations


807  
COURT (ARTS)

807.1 A court is not required in an ARTS zone; however, if a court is provided it shall have the following minimum dimensions:

TABLE K § 807.1:  MINIMUM COURT DIMENSIONS

	Type of Structure
	Minimum Width Open Court
	Minimum Width Closed Court
	Minimum Area Closed Court

	Residential, more than three units:
	4 in./ft. of height of court; 

10 ft. minimum
	4 in./ft. of height of court;

15 ft. minimum
	Twice the square of the required width of court dimension;

350 sq. ft. minimum

	Non-Residential and Lodging:
	2.5 in./ft. of height of court;

6 ft. minimum
	2.5 in./ft. of height of court;

12 ft. minimum
	Twice the square of the required width of court dimension;

250 sq. ft. minimum


SOURCE: Final Rulemaking published at 63 DCR 2447, 3176 (March 4, 2016 – Part 2).
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