775
SIDE YARDS (C)

775.1
Side yards shall be provided for structures in a Commercial District as specified in this section.

775.2
A one-family detached dwelling shall be subject to the side yard requirements of an R-1 District.

775.3
A one-family semi-detached dwelling shall be subject to the side yard requirements of an R-2 District.

775.4
No side yard shall be required for a hotel; but if a side yard is provided, the width of the yard shall be as follows:

(a)
In a C-1, C-2, or C-3-A District: three inches (3 in.) wide for each foot of height of building, but not less than eight feet (8 ft.); and

(b)
In a C-3-B, C-3-C, C-4, or C-5 (PAD) District: two inches (2 in.) wide for each foot of height of building, but not less than six feet (6 ft.).

775.5
No side yard shall be required for any other building or structure; but if a side yard is provided, it shall be at least two inches (2 in.) wide for each foot of height of building, but not less than six feet (6 ft.).


SOURCE: § 5303.4 of the Zoning Regulations, effective May 12, 1958; as amended by Final Rulemaking published at 27 DCR 2226, 2228 (May 23, 1980); and Final Rulemaking published at 47 DCR 9741-43 (December 8, 2000), incorporating by reference the text of Proposed Rulemaking published at 47 DCR 8335, 8412 (October 20, 2000).

