1728
REDUCTION OF REAR YARDS AND SIDE YARDS OF BUILDINGS ABUTTING ALLEYS (DD/MVT)

1728.1
In the event that the Council of the District of Columbia accepts a dedication of land for public alley purposes within DD/MVT that would have been required to be a rear yard pursuant to § 774.7, and the land dedicated is adjacent to a public alley and extends the entire length of the lot, the rear yard requirements for the portion of the structure above the horizontal plane described in § 774.7(a) shall be reduced by five (5) feet for every ten (10) foot depth of land dedicated.

1728.2
For the purposes of § 1728.1, the depth of the land dedicated shall be measured perpendicular to the alignment of the adjacent public alley.

1728.3
In the event that the Council of the District of Columbia accepts a dedication of land for public alley purposes within DD/MVT that would have been required to be a side yard pursuant to §§775.4 and 775.5, and the land dedicated is at least eight (8) feet deep, is adjacent to a public alley, and extends the entire length of the lot, the side yard requirement shall be eliminated for that portion of the structure below a horizontal plane twenty (20) feet above the mean finished grade measured at the middle of the side of the structure.


SOURCE: Final Rulemaking published at 53 DCR 7860 (September 29, 2006).

