District of Columbia Municipal Regulations


M105  
CARBON MONOXIDE DETECTION

M105.1  
General. Carbon monoxide alarms shall be installed in all dwellings used for home day care equipped with a fuel burning appliance or an attached garage.  Carbon monoxide alarms shall be installed in accordance with Section R315.

SOURCE: Final Rulemaking published at 63 DCR 15739 (December 23, 2016).
The District of Columbia Residential Code (2013), referred to as the “Residential Code,” consists of the 2012 edition of the International Residential Code for One- and Two-Family Dwellings, published by the International Code Council (ICC), as amended by the District of Columbia Residential Code Supplement (2013) (12 DCMR B). The International Residential Code is copyrighted by the ICC and therefore is not republished here. However, a copy of the text may be obtained at: http://publicecodes.cyberregs.com/icod/irc/2012/index.htm?bu=IC-P-2012-000002&bu2=IC-P-2012-000019.
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