District of Columbia Municipal Regulations


3011 
REQUIRED ELEVATOR SIGNAGE
Insert new Section 3011 in the Building Code to read as follows:

3011.1 
Required Elevator Signage. A permanent sign of durable material, with lettering no smaller than one quarter inch (6 mm) high shall be placed in all elevators cars, with the following wording:
ALL ACCIDENTS ON OR DAMAGE TO ELEVATORS ARE TO BE REPORTED TO THE DEPARTMENT OF CONSUMER AND REGULATORY AFFAIRS 202 442-4400; OR AFTER WORKING HOURS BY CALLING 311.

SOURCE: Final Rulemaking published at 61 DCR 2782 (March 28, 2014 – Part 2).
The District of Columbia Building Code (2013), referred to as the “Building Code,” consists of the 2012 edition of the International Building Code as amended by the District of Columbia Building Code Supplement (2013)(12  DCMR A). The International Building Code is copyrighted by the International Code Council and therefore is not republished here. However, a copy of the text may be obtained at:
http://publicecodes.cyberregs.com/icod/ibc/2012/index.htm?bu=IC-P-2012-000001&bu2=IC-P-2012-000019.
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