District of Columbia Municipal Regulations


403  
HEIGHT (HE)

403.1 The maximum permitted building height and number of stories, not including the penthouse, in HE shall be given in the following table:

TABLE K § 403.1:  MAXIMUM PERMITTED HEIGHT AND STORIES
	HE Sub-District
	Building Height

Minimum             Maximum
	No. of Stories

	HE-1 (19th St.)
	26 ft.
	50 ft.
	4

	HE-2 (20th St.)
	40 ft.
	80 ft.
	7

	HE-3 (Water St.)
	80 ft.
	110 ft.
	10

	HE-4 (Corrections)
	-
	90 ft.
	8

	Square  E (Park)
	-
	26 ft.
	-


403.2 Building height shall be measured from the lowest curb level along a street frontage abutting the lot.  

403.3 A hospital located in the HE-2 zone may exceed eighty feet (80 ft.) in height, to a maximum of one hundred ten feet (110 ft.), if approved as a special exception by the Zoning Commission pursuant to Subtitle K § 416.

403.4 Penthouses shall be subject to the regulations of Subtitle C, Chapter 15 and the height and story limitations specified in Subtitle K § 403.5.
403.5 The maximum permitted height of a penthouse, except as prohibited on the roof of a detached dwelling, semi-detached dwelling, rowhouse, or flat in Subtitle C §1500.4, shall be as set forth in the following table:

TABLE K § 403.5: MAXIMUM PERMITTED PENTHOUSE HEIGHT AND STORIES

	ZONE DISTRICT
	Maximum Penthouse Height 
	Maximum Penthouse Stories

	HE-1
	12 ft. except 

15 ft. for penthouse mechanical space
	1; second story permitted for penthouse mechanical space

	HE-2
	20 ft.
	1; second story permitted for penthouse mechanical space

	HE-3, HE-4
	20 ft.
	1 plus mezzanine; second story permitted for penthouse mechanical space


403.6 The matter of right height shall serve as the maximum permitted height, penthouse height, and floor area ratio for a PUD.

SOURCE: Final Rulemaking published at 63 DCR 2447, 3176 (March 4, 2016 – Part 2).
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