District of Columbia Municipal Regulations


K105  
CARBON MONOXIDE DETECTION 

K105.1  
General.  Carbon monoxide alarms shall be installed in all home day care occupancies equipped with a fuel burning appliance or an attached garage.  Carbon monoxide alarms shall be installed in accordance with Section R315 of the Residential Code or Section 908.7 of the Fire Code as applicable.

SOURCE: Final Rulemaking published at 63 DCR 15739 (December 23, 2016).

The District of Columbia Fire Code (2013), referred to as the “Fire Code,” consists of the 2012 edition of the International Fire Code  as amended by the District of Columbia Fire Code Supplement (2013) (12 DCMR H).  The International Fire Code is copyrighted by the International Code Council and therefore is not republished here.  However, a copy of the text may be obtained at: http://publicecodes.cyberregs.com/icod/ifc/2012/index.htm?bu=IC-P-2012-000003&bu2=IC-P-2012-000019.
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