District of Columbia Municipal Regulations


403 
MINIMUM PLUMBING FACILITIES
Strike Section 403.4 of the International Plumbing Code in its entirety and insert new Section 403.4 in the Plumbing Code in its place to read as follows:

403.4 
Signage.  Multi-occupancy public facilities shall be designated by a legible sign for each sex.  Single-occupancy public facilities shall be designated with gender-neutral signage.  Signs shall be readily visible and located near the entrance to each toilet facility.  Signs for accessible toilet facilities shall comply with Section 111 of the International Building Code.
SOURCE: Final Rulemaking published at 61 DCR 3169 (March 28, 2014 – Part 2); as corrected by Errata Notice published at 61 DCR 5246 (May 23, 2014).

The District of Columbia Plumbing Code (2013), referred to as the “Plumbing Code,” consists of the 2012 edition of the International Plumbing Code  as amended by the District of Columbia Plumbing Code Supplement (2013) (12 DCMR F). The International Plumbing Code is copyrighted by the International Code Council and therefore is not republished here. However, a copy of the text may be obtained at: http://publicecodes.cyberregs.com/icod/ipc/2012/index.htm?bu=IC-P-2012-000004&bu2=IC-P-2012-000019.
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