District of Columbia Municipal Regulations


701
GENERAL
Strike Section 701.2 of the International Plumbing Code in its entirety and insert new Section 701.2 in the Plumbing Code to read as follows:

701.2 
Sewer required. Buildings in which plumbing fixtures are installed and premises having drainage piping shall be connected to a public sewer where available, or an approved private sewage disposal system.

SOURCE: Final Rulemaking published at 62 DCR 103 (January 2, 2015).
The District of Columbia Plumbing Code (2013), referred to as the “Plumbing Code,” consists of the 2012 edition of the International Plumbing Code  as amended by the District of Columbia Plumbing Code Supplement (2013) (12 DCMR F). The International Plumbing Code is copyrighted by the International Code Council and therefore is not republished here. However, a copy of the text may be obtained at: http://publicecodes.cyberregs.com/icod/ipc/2012/index.htm?bu=IC-P-2012-000004&bu2=IC-P-2012-000019.
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