2301
PARKING GARAGES

2301.1
A building erected, altered, converted, or reconstructed for use as a parking garage shall be subject to the provisions in this section.

2301.2
A parking garage that is an accessory use may be located as follows:

(a)
As an accessory building in any district subject to the general provisions for accessory buildings as specified in § 2500; and

(b)
Within the main building; provided:

(1)
The entrance or exit to the garage shall be accessible and, when it opens onto an alley, the entrance or exit shall be set back at least twelve feet (12 ft.) from the center line of the alley; and

(2)
That portion of the garage beneath a side yard, rear yard, or court shall not obstruct required light and ventilation and shall be designed so that the area above it can be used for an unobstructed level open terrace.

2301.3
A parking garage erected, altered, converted, or reconstructed as a principal use shall have no vehicular entrance or exit nearer than forty feet (40 ft.) to a street intersection as measured from the intersection of the curb lines extended. The entrance or exit to the garage shall be accessible and, when it opens onto an alley, the entrance or exit shall be set back at least twelve feet (12 ft.) from the center line of the alley.
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