District of Columbia Municipal Regulations


P2908
DRINKING WATER TREATMENT UNITS

Strike Section P2908.1 of the International Residential Code in its entirety and insert new Section P2908.1 in the Residential Code in its place to read as follows:

P2908.1 
Design.  Drinking water treatment units shall meet the requirements of NSF 42, NSF 44, NSF 53, NSF 62 or CSA B483.1.

SOURCE: Final Rulemaking published at 61 DCR 3063 (March 28, 2014 – Part 2). 
The District of Columbia Residential Code (2013), referred to as the “Residential Code,” consists of the 2012 edition of the International Residential Code for One- and Two-Family Dwellings, published by the International Code Council (ICC), as amended by the District of Columbia Residential Code Supplement (2013) (12 DCMR B). The International Residential Code is copyrighted by the ICC and therefore is not republished here. However, a copy of the text may be obtained at: http://publicecodes.cyberregs.com/icod/irc/2012/index.htm?bu=IC-P-2012-000002&bu2=IC-P-2012-000019.
	
	Residential Code Supplement of 2013
12-B DCMR § P2908

	

	
	
	



