District of Columbia Municipal Regulations


4401 
ASTM

ASTM International

100 Barr Harbor

West Conshohocken, PA 19428-2959

Insert a new standard references in Chapter 44 of the Residential Code under subheading ASTM to read as follows:

	Standard 

reference number
	Title
	Referenced in code section number

	E408-71 (2008) 


	Standard Test Methods for Total Normal Emittance of Surfaces Using Inspection-Meter Techniques


	R908.2

	C1549-09 


	Standard Test Method for Determination of Solar Reflectance Near Ambient Temperature Using a Portable Solar Reflectometer
	R908.2

	C 1371-04a 
	Standard Test Method for Determination of Emittance of Materials Near Room Temperature Using Portable Emissometers
	R908.2

	E1980-11 


	Standard Practice for Calculating Solar Reflectance Index of Horizontal and Low-Sloped Opaque Surfaces
	R908.2

	E1918-06
	Standard Test Method for Measuring Solar Reflectance of Horizontal and Low-Sloped Surfaces in the Field
	R908.2


SOURCE: Final Rulemaking published at 61 DCR 3063 (March 28, 2014 – Part 2). 
The District of Columbia Residential Code (2013), referred to as the “Residential Code,” consists of the 2012 edition of the International Residential Code for One- and Two-Family Dwellings, published by the International Code Council (ICC), as amended by the District of Columbia Residential Code Supplement (2013) (12 DCMR B). The International Residential Code is copyrighted by the ICC and therefore is not republished here. However, a copy of the text may be obtained at: http://publicecodes.cyberregs.com/icod/irc/2012/index.htm?bu=IC-P-2012-000002&bu2=IC-P-2012-000019.
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