District of Columbia Municipal Regulations


601
GENERAL

Strike Section 601.3.1 in the International Green Construction Code in its entirety and insert new Section 601.3.1 in the Green Construction Code in its place to read as follows:

601.3.1 Performance-based compliance.  Buildings designed on a performance basis shall comply with Sections 602, 608.6, 609, and 611.

Strike Section 601.3.2 of the International Green Construction Code in its entirety and insert new Section 601.3.2 in the Green Construction Code in its place to read as follows:

601.3.2 Prescriptive-based compliance.  Buildings designed on a prescriptive basis shall comply with the requirements of Sections 605, 606, 607, 608, 609, and 611. 

SOURCE: Final Rulemaking published at 61 DCR 3356 (March 28, 2014 – Part 2); as corrected by Errata Notice published at 61 DCR 5246 (May 23, 2014).

The District of Columbia Green Construction Code (2013) , referred to as the “Green Construction Code,” consists of the 2012 edition of the International Green Construction Code published by the International Code Council (ICC), as amended by the District of Columbia Green Construction Code Supplement (2013)(12 DCMR K).  The International Green Construction Code is copyrighted by the International Code Council and therefore is not republished here.  However, a copy of the text may be obtained at:
http://publicecodes.cyberregs.com/icod/igcc/2012/index.htm?bu=IC-P-2012-000023&bu2=IC-P-2012-000019. 
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